{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["拟购仪器","拟购试剂"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"拟购仪器","index":0,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,1,0,7]],"flags":["formulas_cached_only"]}
[null,"滑县2013年测土配方施肥项目土壤样品化验试剂、仪器购置清单"]
["序号","名称","规格","单位","数量","单价","总额","备注"]
[115,"台式PH计","F-33 型","台",1,null,null,"Ph测量范围：-2.00pH～16.00 pH，分辨率：0.01 pH，准确度：± 0.01 pH，mV测量范围：±1999.9 mV，分辨率：0.1 mV，准确度：± 0.05 读数± 1字，℃测量范围：-10℃～+110 ℃，分辨率：0.1℃；≥100℃，1.0℃，准确度：±0.5℃；≥100℃,1.0℃，pH校正方式：1点或2点自动校正，自动缓冲液识别：1.68、4.00、6.86、9.18、12.45 (25.0℃)，电极参数保存：自动存储，温度补偿：自动/手动 0℃-100℃，内部时钟(注)：实时时钟，RS232接口：有 9600波特率，配套电极：E-900型，配套缓冲液：4.00、6.86、9.18"]
[116,"紫外可见分光光度计","T6S新世纪","台",1,null,null,"性能指标：波长范围：190nm～1100nm，波长准确度：±1nm(开机自动校准)，\n*波长重复性：≤0.2nm，光谱带宽：2.0nm，*杂散光： <0.05%T(220nm,NaI; 340nm,NaNo2)，光度方式：透过率，吸光度，能量，光度范围：-0.3～3.0Abs，\n*光度准确度：±0.002Abs(0～0.5Abs),  ±0.004Abs(0.5～1.0Abs)；±0.3%T(0～100%T)，光度重复性：≤0.001Abs(0～0.5Abs), 　≤0.002Abs(0.5～1.0Abs)；　≤0.15%T(0～100%T)，基线平直度：±0.002Abs(200nm～1100nm)，*基线漂移：≤0.001Abs/h(500nm, 0Abs预热2小时后)，光度噪声：±0.001Abs(500nm,0Abs )\n"]
[117,"低速离心机","SC-3610","台",1,null,null,"技术指标：最高转速Max peed 6000rpm， 最大相对离心力Max RCF 5000×g ， 转速精度Speed accuracy ±20rpm，转子最大容量Rotor capacity 100ml×4， 温升指标Temperature rise ≤10℃（运行20分钟），噪 音Noise ≤65dB ，定时范围Timer range 1～9999min/连续/点动 ， 结 构Construction 钢制结构，不锈钢离心腔，重量Weight 51kg，外形尺寸Dimensions 430×500×415 mm （L×W×H）。 "]
[118,"自动凯氏定氮仪","SPD50","台",1,null,null,"检测范围：0.1~200mgN， 样品量：5g,15ml ，蒸馏速度：＜5min/样品 ， 回收率：≥99.5%，重复率：≤1%     水压：0.15Mpa ，冷却水用量：0.5-1L/min ，供电220V，50HZ功率：1500W ，外形尺寸：400×400×640mm  ，重量：20kg。"]
[119,"水浴恒温振荡器","SHA-C","台",1,null,null,"使用电源：220V.50Hz ，整机功率：1580W，定时范围 ：5～120min ，振荡频率；启动～300r/min，振荡幅度：20mm ，恒温范围：常温－100℃±1.0。"]
[null,"控制最高限价",{"$nulls":4},97000]

{"sheet":"拟购试剂","index":1,"n_rows":116,"n_cols":8,"rows_kept":116,"cut":false,"hidden":false,"merged":[[0,1,0,7]],"flags":["formulas_cached_only"]}
[null,"滑县2013年测土配方施肥项目土壤样品化验试剂、仪器购置清单"]
["序号","名称","规格","单位","数量","单价","总额","备注"]
[1,"阿拉伯胶（优级）","   GR250g","瓶",5,null,null,"上海国药"]
[2,"高锰酸钾","AR500g"," 瓶",1,null,null,"上海国药"]
[3,"钼酸钠","AR500g"," 瓶",5,null,null,"上海国药"]
[4,"氯化钾","GR500g"," 瓶",1,null,null,"上海国药"]
[5,"硫酸镁","GR500g"," 瓶",1,null,null,"上海国药"]
[6,"抗坏血酸","25g"," 瓶",40,null,null,"上海国药"]
[7,"硼酸（优级）","500g"," 瓶",50,null,null,"上海国药"]
[8,"硫酸亚铁铵","AR500g"," 瓶",20,null,null,"上海国药"]
[9,"氢氧化钠","AR500g"," 瓶",100,null,null,"上海国药"]
[10,"硫酸","GR500ml"," 瓶",40,null,null,"北化"]
[11,"硫酸","AR500ml"," 瓶",80,null,null,"北化"]
[12,"盐酸","AR500ml"," 瓶",20,null,null,"北化"]
[13,"盐酸（优级）","  GR500ml"," 瓶",20,null,null,"北化"]
[14,"氨水（优级）","   GR500"," 瓶",20,null,null,"北化"]
[15,"硝酸（优级）","  GR500ml"," 瓶",20,null,null,"北化"]
[16,"氯化钙（无水）","AR500g","瓶",1,null,null,"上海国药"]
[17,"氯化钡晶粒","AR500g","瓶",10,null,null,"上海国药"]
[18,"氯化铵","AR500g","瓶",2,null,null,"上海国药"]
[19,"溴甲酚绿指示剂","10g","瓶",1,null,null,"上海国药"]
[20,"PH缓冲溶液",null,null,5,null,null,"上海雷磁"]
[21,"乙醇95%","AR500ml","瓶",100,null,null,"北化"]
[22,"钙鎂指示剂",null,"瓶",2,null,null,"上海阿拉丁"]
[23,"酚酞","25g","瓶",1,null,null,"上海国药"]
[24,"无水乙醇","AR500ml","瓶",40,null,null,"北化"]
[25,"重铬酸钾","AR500g","瓶",20,null,null,"北化"]
[26,"硫酸亚铁铵","AR500g","瓶",20,null,null,"北化"]
[27,"汞（优级）","AR250ml","瓶",2,null,null,"北化"]
[28,"玛瑙研钵","直径8-12cm","个",1,null,null,"贵州"]
[29,"ph标准物质",null,"套",50,null,null,"上海雷磁"]
[30,"硝酸","GR500ml","瓶",20,null,null,"北化"]
[31,"无水甲醇","500ml"," 瓶",40,null,null,"北化"]
[32,"氟化铵","500g"," 瓶",40,null,null,"北化"]
[33,"甲醛","500g"," 瓶",20,null,null,"北化"]
[34,"乙二醇","500ml"," 瓶",40,null,null,"上海国药"]
[35,"醋酸钠","500g"," 瓶",100,null,null,"上海国药"]
[36,"次氯酸钠","500g"," 瓶",20,null,null,"上海国药"]
[37,"氯化钙（基准）分析","500g"," 瓶",20,null,null,"北化"]
[38,"三乙醇胺","AR500ml"," 瓶",40,null,null,"北化"]
[39,"氯化钙","AR500g"," 瓶",40,null,null,"北化"]
[40,"草酸铵","GR500g"," 瓶",60,null,null,"上海国药"]
[41,"草酸","500g"," 瓶",60,null,null,"上海国药"]
[42,"苯羟乙酸","25g"," 瓶",20,null,null,"上海三爱思"]
[43,"氯酸钾","500g"," 瓶",20,null,null,"北化"]
[44,"硫酸铜","500g"," 瓶",80,null,null,"北化"]
[45,"无水碳酸钠","500g"," 瓶",100,null,null,"北化"]
[46,"二乙三胺五乙酸","25g"," 瓶",40,null,null,"上海三爱思"]
[47,"盐酸","AR500ml"," 瓶",100,null,null,"北化"]
[48,"乙醇","AR500ml"," 瓶",100,null,null,"上海国药"]
[49,"硫酸锰","500g"," 瓶",80,null,null,"上海国药"]
[50,"氨水","AR500ml","瓶",100,null,null,"北化"]
[51,"乙酸铵","AR500g","瓶",80,null,null,"北化"]
[52,"高氯酸","AR500ml","瓶",40,null,null,"北化"]
[53,"柠檬酸","AR500g","瓶",80,null,null,"上海国药"]
[54,"乙二铵四乙酸二钠","AR500g","瓶",100,null,null,"上海国药"]
[55,"喹啉","AR500g","瓶",10,null,null,"上海国药"]
[56,"变色硅胶","AR500g","瓶",60,null,null,"青岛海化"]
[57,"丙三醇","AR500g","瓶",80,null,null,"上海国药"]
[58,"四苯硼钠","AR10g","瓶",1,null,null,"上海三爱思"]
[59,"溴水","AR500ml","瓶",20,null,null,"北化"]
[60,"乙炔气体",null,"瓶",6,null,null,"北普"]
[61,"标准土样","潮土 500g","瓶",1,null,null,"国家标物中心"]
[62,"去污粉",null,"件",5,null,null,"郑州"]
[63,"广泛PH试纸",null,"个",50,null,null,"上海三爱思"]
[64,"科邦橡胶医用手套",null,"双",50,null,null,"广东"]
[65,"工业耐酸碱牛筋手套","大码","双",40,null,null,"南洋牌"]
[66,"乳胶管(厚)","0.5cm","袋",4]
[67,"滤纸（定量）","直径12.5cm","盒",300,null,null,"杭州特种纸业有限公司"]
[68,"小烧杯","25ml","个",100,null,null,"北京玻璃仪器厂"]
[69,"烧杯","50ml","个",80,null,null,"北京玻璃仪器厂"]
[70,"烧杯（高型）","100ml","个",60,null,null,"北京玻璃仪器厂"]
[71,"烧杯","100ml","个",80,null,null,"北京玻璃仪器厂"]
[72,"烧杯","500ml","个",20,null,null,"北京玻璃仪器厂"]
[73,"烧杯","1000ml","个",10,null,null,"北京玻璃仪器厂"]
[74,"烧杯","2000ml","个",6,null,null,"北京玻璃仪器厂"]
[75,"烧杯","3000ml","个",10,null,null,"北京玻璃仪器厂"]
[76,"烧杯","5000ml","个",10,null,null,"北京玻璃仪器厂"]
[77,"容量瓶","1000ml","个",10,null,null,"北京玻璃仪器厂"]
[78,"容量瓶","50ml","只",50,null,null,"北京玻璃仪器厂"]
[79,"容量瓶","100ml","只",50,null,null,"北京玻璃仪器厂"]
[80,"容量瓶","2000ml","只",8,null,null,"北京玻璃仪器厂"]
[81,"半自动滴定管","50ml","只",2,null,null,"北玻"]
[82,"复合电极","F-33C PH/MV10C","个",2,null,null,"上海雷磁"]
[83,"称量勺",null,"个",5,null,null,"广东"]
[84,"玻璃棒",null,"根",20,null,null,"广东"]
[85,"吸管（胖度）","10ml","根",10,null,null,"北玻"]
[86,"吸管（胖度）","25ml","根",5,null,null,"北玻"]
[87,"吸管（胖度）","50ml","根",6,null,null,"北玻"]
[88,"滴瓶（棕色）","50ml","个",10,null,null,"北玻"]
[89,"耐酸碱手套",null,"双",18,null,null,"广东"]
[90,"容量瓶","2000ml","个",6,null,null,"北玻"]
[91,"电炉","2KW","个",4,null,null,"北京"]
[92,"电炉","1KW","个",2,null,null,"北京"]
[93,"双联电炉","1KW","个",2,null,null,"北京"]
[94,"电炉丝","1KW","根",5,null,null,"北京"]
[95,"电炉丝","5KW","根",5,null,null,"北京"]
[96,"毛刷（消化管）","42*250","根",20,null,null,"冀州耀华"]
[97,"毛刷（试管）","20*250","根",20,null,null,"冀州耀华"]
[98,"毛刷（试管）","40*400","根",20,null,null,"冀州耀华"]
[99,"毛刷（吸管）",null,"根",10,null,null,"冀州耀华"]
[100,"离心机","SC-3610 ","台",1,null,null,"每分钟3000-5000转"]
[101,"离心管","100ml","个",30,null,null,"湖南"]
[102,"滴定管（碱式）","25ml","只",3,null,null,"北玻"]
[103,"滴定管（碱式）","50ml","只",3,null,null,"北玻"]
[104,"滴定架",null,"套",2,null,null,"冀州耀华"]
[105,"胶塞","5#","个",20,null,null,"武汉解放"]
[106,"称量纸","大","包",6,null,null,"上海"]
[107,"称量纸","小","包",6,null,null,"上海"]
[108,"漏斗","75mm","个",56,null,null,"申玻"]
[109,"帯盖放盘",null,"个",4,null,null,"上海白鹅"]
[110,"镊子",null,"把",2,null,null,"广东"]
[111,"Cu标液","1000ug/ml  20ml","瓶",3,null,null,"国家标准物质中心每瓶50ml"]
[112,"Zn标液","1000ug/ml  20ml","瓶",1,null,null,"国家标准物质中心每瓶50ml"]
[113,"Mn标液","1000ug/ml  20ml","瓶",2,null,null,"国家标准物质中心每瓶50ml"]
[114,"Fe标液","1000ug/ml  20ml","瓶",2,null,null,"国家标准物质中心每瓶50ml"]