{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,0,0,6],[45,0,45,1],[47,0,48,6]],"flags":["formulas_cached_only"]}
["2013年全国基层农技推广示范县项目                           水肥一体化灌溉系统设备预算表"]
["序号","材料名称","规格型号","单位","数量","单价","合价（元）"]
["一","管道工程",{"$nulls":4},4200]
["1","土方开挖",null,"m",700,4,2800]
["2","土方回填",null,"m",700,2,1400]
[]
["二","首部控制",{"$nulls":4},56067]
[1,"储肥罐（304材质）","200L","套",2,3500,7000]
[2,"网式过滤器 80 目","3/4\" ","个",2,181,362]
[3,"空气阀(以色列）","2\" ","个",2,920,1840]
[4," 叠片过滤器 "," 3\"(120 目)","个",4,2350,9400]
[5,"PVC管","φ40","米",167,13,2171]
[6,"PVC管","φ90/10","米",700,27,18900]
[7,"快速释压阀(以色列）","2\"","个",2,1730,3460]
[8," 逆止阀","3.5〞","个",2,600,1200]
[9," 蝶阀（齿轮、直柄各一个）","3.5〞","个",4,360,1440]
[10,"水表","3.5〞","个",2,650,1300]
[11,"PVC活套法兰","3.5〞","个",8,56,448]
[12,"法兰（焊接、带螺栓、垫片）","3.5〞","片",2,113,226]
[13,"铜三通"," 3/4\" ","个",8,27,216]
[14,"压力表（带弯管）","3/4“*1.6Pa","个",4,65,260]
[15,"转换接头","3\"*90(卡口）","个",8,306,2448]
[16,"PVC接头","（63*2\"外丝）","个",4,27,108]
[17,"PVC弯头","φ90","个",4,13,52]
[18,"PVC三通","φ90","个",4,50,200]
[19,"PVC三通","φ90×40","个",167,28,4676]
[21,"PVC 三通","φ90*32","个",12,16,192]
[22,"PVC变径","φ32*25","个",8,5,40]
[23,"PVC变径","φ32*3/4”","个",8,4,32]
[24,"PVC变径","φ63*32","个",8,12,96]
[]
["三","管件部分",{"$nulls":4},43094]
[1,"PVC法兰(含螺栓)","φ90","套",2,115,230]
[2,"PVC 90度弯头","φ90","个",4,13,52]
[3,"PVC 三通","φ90","个",4,50,200]
[4,"球阀","φ90","个",4,127,508]
[5,"球阀","φ40","个",167,32,5344]
[6,"空气阀","2\"","个",4,920,3680]
[7,"PVC 接头(内丝）","φ90×40","个",24,42,1008]
[8,"PVC堵头","φ90","个",4,30,120]
[9,"PVC胶水","1Kg/桶","Kg",8,34,272]
[10,"微喷带","50〃","米",17600,1.8,31680]
[]
["四","运费",{"$nulls":4},2500]
["五","安装费",{"$nulls":4},10000]
["合     计",{"$nulls":5},115861]
[]
["要求：中标企业对水肥一体化灌溉系统进行免费设计、安装、调试，管件上印上实施单位名称"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}